

AWS Current-State Configuration

Account ID:

Account Alias:

American Express Global Business Travel

SOW# 00007620

Architecture Assessment

**Deliver To:**

Neil Kirk

VP – Global Technology Services Platform Engineering and Technology

**Prepared By:**

Computacenter US

AJ Cruz, CCIE 50268

Principal Consultant

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| One University Ave,  Suite 102  Westwood, MA 02090 |  | p. 714-861-2200 |  | www.computacenter.com |

Table of Contents

1. [Document Control 3](#_Toc131827692)
2. [Introduction 4](#_Toc131827693)

[Document Overview](#_Toc131827694)

1. [AWS Account Dashboard 4](#_Toc131827695)
2. [Best Practices & Health Static Auto-Analysis 4](#_Toc131827696)

[Transit Gateway Analysis](#_Toc131827697)

[VPN Analysis](#_Toc131827698)

[VPC Analysis](#_Toc131827699)

[Load Balancer Analysis](#_Toc131827700)

[EC2 instance Analysis](#_Toc131827701)

1. [VPCs 5](#_Toc131827702)
2. [Route Tables 5](#_Toc131827703)
3. [Route Tables - Routes 5](#_Toc131827704)
4. [Prefix Lists 5](#_Toc131827705)
5. [Subnets 5](#_Toc131827706)
6. [Network ACLs 5](#_Toc131827707)
7. [Network ACL – Inbound Entries 5](#_Toc131827708)
8. [Network ACL – Outbound Entries 5](#_Toc131827709)
9. [Security Groups 5](#_Toc131827710)
10. [Security Group – Inbound Entries 6](#_Toc131827711)
11. [Security Group – Outbound Entries 6](#_Toc131827712)
12. [Internet Gateways 6](#_Toc131827713)
13. [Egress-Only Internet Gateways 6](#_Toc131827714)
14. [NAT Gateways 6](#_Toc131827715)
15. [Endpoint Services 6](#_Toc131827716)
16. [Endpoints 6](#_Toc131827717)
17. [Peering Connections 6](#_Toc131827718)
18. [Transit Gateways 6](#_Toc131827719)
19. [Transit Gateway Routes 7](#_Toc131827720)
20. [VPN – Customer Gateways 7](#_Toc131827721)
21. [VPN – Site-to-Site Connections (Connected to Transit Gateways) 7](#_Toc131827722)
22. [VPN – Virtual Private Gateways 7](#_Toc131827723)
23. [Direct Connect Gateways 7](#_Toc131827724)
24. [Load Balancers 7](#_Toc131827725)
25. [Load Balancer Target Groups 7](#_Toc131827726)
26. [EC2 Instances 7](#_Toc131827727)

# Document Control

**Preparation**

|  |  |  |
| --- | --- | --- |
| ****Action**** | ****Name**** | ****Date**** |
| Technical Content & Formatting | [Engineer’s Name] | 7/2/2015 |

**Release**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Version | ****Date Released**** | Change Notice | Pages Affected | ****Remarks**** |
| 1.00 | 7/2/2015 | All | All | Initial release |

**Distribution List**

|  |  |  |  |
| --- | --- | --- | --- |
| ****Name**** | ****Organization**** | ****Role**** | ****E-mail**** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Introduction

GBT has engaged Computacenter US to provide consulting services to assess GBT’s network architecture and configuration to provide recommendations and a roadmap to optimize and stabilize the environment.

## Document Overview

This document captures the current network configuration of an AWS account (identified on the title page and the account dashboard below). All data is gathered via the AWS API using the Python Boto3 client.

Additionally, data returned by the API is used to auto-generate some basic best-practices analysis as well as health status of various objects (VPN connections, etc.)

Amazon-published best practices are used for reference:

* <https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html>
* <https://docs.aws.amazon.com/vpc/latest/userguide/vpc-security-best-practices.html>
* <https://aws.amazon.com/blogs/networking-and-content-delivery/best-practices-for-deploying-gateway-load-balancer/>
* <https://docs.aws.amazon.com/AWSEC2/latest/UserGuide/enhanced-networking.html>

# AWS Account Dashboard

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ACCOUNT ID | 195750747780 | | ACCOUNT ALIAS | gbtcloud-transit-use1-195750747780 | |
| REGIONS IN USE | eu-west-1 us-east-1 us-west-2 | | EC2/VPC COUNT | 24 EC2 instances across 6 VPCs | |
| TRANSIT GATEWAY ANALYSIS | | VPN ANALYSIS | VPC ANALYSIS | LOAD BALANCER ANALYSIS | EC2 INST ANALYSIS |
| 5 of 5 checks passed. | | 0 of 0 checks passed. | 2 of 2 checks passed. | 0 of 1 checks passed. | 1 of 1 checks passed. |

# Best Practices & Health Static Auto-Analysis

## Transit Gateway Analysis

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | TGW PER-REGION QUANTITY CHECK: PASS | | | | | | TEST DESCRIPTION | Because Transit Gateways are highly available by design, multiple gateways per region are not required for high availability. https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html | | | | | RESULT DETAILS | All regions have no more than one Transit Gateway. | | | | |
|  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | UNIQUE BGP ASN CHECK: PASS | | | | | | TEST DESCRIPTION | For deployments with multiple transit gateways, a unique Autonomous System Number (ASN) for each transit gateway is recommended. https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html | | | | | RESULT DETAILS | All Transit Gateway ASNs are unique. | | | | |
|  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | ONE NET ACL FOR ATTACHMENT SUBNETS CHECK: PASS | | | | | | TEST DESCRIPTION | Create one network ACL and associate it with all of the subnets that are associated with the transit gateway. https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html | | | | | RESULT DETAILS | All Transit Gateway VPC Attachment Subnets are in a single Network ACL. | | | | |
|  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | NET ACL OPEN CHECK: PASS | | | | | | TEST DESCRIPTION | Create one network ACL and associate it with all of the subnets that are associated with the transit gateway. Keep the network ACL open in both the inbound and outbound directions. https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html | | | | | RESULT DETAILS | All Transit Gateway VPC Attachment Subnet Network ACLs are open. | | | | |
|  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | VPN ATTACHMENT BGP CHECK: PASS | | | | | | TEST DESCRIPTION | Use Border Gateway Protocol (BGP) Site-to-Site VPN connections. https://docs.aws.amazon.com/vpc/latest/tgw/tgw-best-design-practices.html | | | | | RESULT DETAILS | All Transit Gateway VPN connections are learning routes dynamically (BGP enabled). | | | | |

## VPN Analysis

|  |
| --- |
| No VPNs Present |

## VPC Analysis

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | EMPTY VPC CHECK: PASS | | | | | | TEST DESCRIPTION | Report any VPCs with no EC2 instances. | | | | | RESULT DETAILS | All VPCs have at least one EC2 instance. | | | | |
|  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | MULTI-AZ VPC CHECK: PASS | | | | | | TEST DESCRIPTION | When you add subnets to your VPC to host your application, create them in multiple Availability Zones. https://docs.aws.amazon.com/vpc/latest/userguide/vpc-security-best-practices.html | | | | | RESULT DETAILS | All VPCs have subnets in two or more Availability Zones. | | | | |

## Load Balancer Analysis

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | LB TARGET HEALTH CHECK: FAIL | | | | | | TEST DESCRIPTION | Report any Load Balancers with Targets in Unhealthy State. | | | | | RESULT DETAILS | The following Load Balancer Targets are in an unhealthy state: us-west-2/vpc-06b2af15774b0380c(vpc-egress-east-west-TransitVPC)/i-00b7cba754dfc68b4 | | | | |

## EC2 instance Analysis

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | ENA SUPPORT ENABLED CHECK: PASS | | | | | | TEST DESCRIPTION | Amazon EC2 provides enhanced networking capabilities through the Elastic Network Adapter (ENA). To use enhanced networking, you must install the required ENA module and enable ENA support. https://docs.aws.amazon.com/AWSEC2/latest/UserGuide/enhanced-networking-ena.html | | | | | RESULT DETAILS | All EC2 instances have ENA Support enabled. | | | | |

# VPCs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| REGION | VPC NAME | VPC CIDR | VPC ID | INSTANCE QTY |
| eu-west-1 | vpc-egress-east-west-TransitVPC | 10.206.0.0/22 | vpc-02eba02cbd3357bd7 | 3 |
| eu-west-1 | vpc-ingress-TransitVPC | 10.206.4.0/22 | vpc-0474c0100ce5e4d3f | 3 |
| us-east-1 | vpc-ingress-TransitVPC | 10.201.4.0/22 | vpc-09ce0acd298aa0180 | 4 |
| us-east-1 | vpc-egress-east-west-TransitVPC | 10.201.0.0/22 | vpc-00a0fc500fad24c91 | 8 |
| us-west-2 | vpc-ingress-TransitVPC | 10.228.4.0/22 | vpc-02745e1fd5db35884 | 3 |
| us-west-2 | vpc-egress-east-west-TransitVPC | 10.228.0.0/22 | vpc-06b2af15774b0380c | 3 |

# Route Tables

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | | gbtcloud-transit-egress-east-west-euw1-tgw-az3 | rtb-06f34c0fd71f7f82f | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-public-az1 | rtb-0e36665306abe2a08 | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-data-az2 | rtb-017e35f2e59206196 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-public-az2 | rtb-0ddc5998187759fe8 | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-tgw-az2 | rtb-0cbda1054025672fb | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-mgmt-az2 | rtb-033fc266c592aec05 | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-gwlbe-az2 | rtb-081eb9730ab875a17 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-tgw-az1 | rtb-0e3bd694abe5fedd4 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-data-az3 | rtb-0ac72e591abc7ed37 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-public-az3 | rtb-03352845967b57f01 | 3 | 1 | 0 |  | |  | rtb-06220418ed077d525 | 1 | 0 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-gwlbe-az3 | rtb-08ca7f2074ec9d229 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-gwlbe-az1 | rtb-064b343b8c5a6a8b2 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-data-az1 | rtb-03fe2a41e26fda7cc | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-mgmt-az3 | rtb-0f999eb741339a2de | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-euw1-mgmt-az1 | rtb-07c1d78423620f600 | 5 | 1 | 0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | |  | rtb-0390e1de75d723f69 | 1 | 0 | 0 |  | | gbtcloud-transit-ingress-euw1-data-az3 | rtb-05680d7a934638399 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-data-az1 | rtb-0865f8e81a686db9c | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-tgw-az2 | rtb-0d4f8906a3285eb73 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-tgw-az1 | rtb-09d4fb237eb379200 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-tgw-az3 | rtb-073f5d2b17550b9aa | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-mgmt-az2 | rtb-0b716323014029275 | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-mgmt-az1 | rtb-0d9db8094db8d3d9f | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-data-az2 | rtb-0ee9cc74fd1dc13a4 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-euw1-mgmt-az3 | rtb-033b68bbf0d4e5449 | 2 | 1 | 0 |  | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | | gbtcloud-transit-ingress-use1-mgmt-az3 | rtb-07e7d4ec3f1375ca6 | 2 | 1 | 0 |  | |  | rtb-0ef28ce638540e84a | 1 | 0 | 0 |  | | gbtcloud-transit-ingress-use1-mgmt-az1 | rtb-0eee5939c97efa4e4 | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-tgw-az2 | rtb-016d95d5808e9bbf5 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-data-az2 | rtb-000195c790a633e47 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-data-az3 | rtb-00e50170ccae7626d | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-mgmt-az2 | rtb-09621ae7c7ba3d852 | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-tgw-az1 | rtb-0ca7ddd0d9035b389 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-tgw-az3 | rtb-0ee75094a5c9892d4 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-use1-data-az1 | rtb-02734e8fb3ce20530 | 1 | 1 | 0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | | gbtcloud-transit-egress-east-west-use1-tgw-az1 | rtb-038a489cf0450c845 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-tgw-az3 | rtb-0fae1ce966892e031 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-gwlbe-az3 | rtb-05d6f92dc60058c21 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-data-az3 | rtb-0d704f8fa8af0323c | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-mgmt-az2 | rtb-0f38ffe8ca43a69b6 | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-public-az3 | rtb-0cd9e7ab8d2f7441d | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-gwlbe-az2 | rtb-08438ea08c40719ee | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-public-az1 | rtb-07570b9770cc42df2 | 3 | 1 | 0 |  | |  | rtb-08eadc94948e477f4 | 1 | 0 | 0 |  | | gbtcloud-transit-egress-east-west-use1-tgw-az2 | rtb-0dd628b462e768da0 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-data-az1 | rtb-050773951feba8070 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-data-az2 | rtb-08a60efbe3e867657 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-public-az2 | rtb-0d0ddc98eb5ec241f | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-gwlbe-az1 | rtb-0e9b943222cdd3b59 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-mgmt-az1 | rtb-0dfca6838fb46ad87 | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-use1-mgmt-az3 | rtb-0a145b986c8ad6006 | 5 | 1 | 0 |  | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | | gbtcloud-transit-ingress-usw2-data-az3 | rtb-00000639405f588ed | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-data-az2 | rtb-03d32f483551ce73a | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-mgmt-az3 | rtb-063f6851247452e3d | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-mgmt-az1 | rtb-0d9200f9ac56fa654 | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-mgmt-az2 | rtb-00b0ed610ae9b5426 | 2 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-tgw-az3 | rtb-05ccbd32bb791795c | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-data-az1 | rtb-073fd47c51650f724 | 1 | 1 | 0 |  | | gbtcloud-transit-ingress-usw2-tgw-az2 | rtb-065544fb1d06e9d22 | 1 | 1 | 0 |  | |  | rtb-01af00f61f711ee5a | 1 | 0 | 0 |  | | gbtcloud-transit-ingress-usw2-tgw-az1 | rtb-0d3ab06f1b767a1ff | 1 | 1 | 0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | RT NAME | RT ID | ROUTE QTY | SUB ASSOC QTY | EDGE ASSOC QTY | ROUTE PROPAGATIONS | | gbtcloud-transit-egress-east-west-usw2-public-az2 | rtb-080f6ad9a7a9b16b4 | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-data-az2 | rtb-09d5eb639d5191b57 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-mgmt-az1 | rtb-0d3f00818765398b7 | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-gwlbe-az2 | rtb-07a36eac2d2effc0f | 4 | 1 | 0 |  | |  | rtb-04b0af9d13718e879 | 1 | 0 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-public-az3 | rtb-07695129fc1f7db68 | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-tgw-az3 | rtb-02a47bffbff43ca04 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-gwlbe-az1 | rtb-0fbc4ebe7f4825d8c | 4 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-data-az1 | rtb-05454afe4c4b7bf09 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-public-az1 | rtb-091fa484a63bd1a1d | 3 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-mgmt-az2 | rtb-03ebbdf0f2d83399f | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-data-az3 | rtb-0cd2fe1df261c2112 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-tgw-az2 | rtb-07030a424dfe630c8 | 2 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-mgmt-az3 | rtb-0bfac5a4517f28b00 | 5 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-gwlbe-az3 | rtb-05b2f7cb9e4c3b63d | 4 | 1 | 0 |  | | gbtcloud-transit-egress-east-west-usw2-tgw-az1 | rtb-0eaddfd6842b09eab | 2 | 1 | 0 |  | |

# Route Tables - Routes

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-tgw-az3 (rtb-06f34c0fd71f7f82f) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-07d638db429bebe5a | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-public-az1 (rtb-0e36665306abe2a08) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-01a6711f8ce1612df | CreateRoute | | pl-6da54004 | vpce-02050004a100a4b5e | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-data-az2 (rtb-017e35f2e59206196) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-public-az2 (rtb-0ddc5998187759fe8) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-01a6711f8ce1612df | CreateRoute | | pl-6da54004 | vpce-02050004a100a4b5e | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-tgw-az2 (rtb-0cbda1054025672fb) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-024f07b53c9e97eb0 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-mgmt-az2 (rtb-033fc266c592aec05) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 172.16.0.0/12 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 10.0.0.0/8 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-gwlbe-az2 (rtb-081eb9730ab875a17) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-tgw-az1 (rtb-0e3bd694abe5fedd4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-001d9d5aad8465874 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-data-az3 (rtb-0ac72e591abc7ed37) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-public-az3 (rtb-03352845967b57f01) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-01a6711f8ce1612df | CreateRoute | | pl-6da54004 | vpce-02050004a100a4b5e | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: <unnamed> (rtb-06220418ed077d525) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-gwlbe-az3 (rtb-08ca7f2074ec9d229) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-gwlbe-az1 (rtb-064b343b8c5a6a8b2) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-data-az1 (rtb-03fe2a41e26fda7cc) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-mgmt-az3 (rtb-0f999eb741339a2de) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 172.16.0.0/12 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 10.0.0.0/8 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-euw1-mgmt-az1 (rtb-07c1d78423620f600) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 172.16.0.0/12 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 10.0.0.0/8 | tgw-0ad502a1c2efd4cf8 | CreateRoute | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: <unnamed> (rtb-0390e1de75d723f69) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-data-az3 (rtb-05680d7a934638399) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-data-az1 (rtb-0865f8e81a686db9c) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-tgw-az2 (rtb-0d4f8906a3285eb73) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-tgw-az1 (rtb-09d4fb237eb379200) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-tgw-az3 (rtb-073f5d2b17550b9aa) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-mgmt-az2 (rtb-0b716323014029275) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-mgmt-az1 (rtb-0d9db8094db8d3d9f) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-data-az2 (rtb-0ee9cc74fd1dc13a4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-euw1-mgmt-az3 (rtb-033b68bbf0d4e5449) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.206.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-0ad502a1c2efd4cf8 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-mgmt-az3 (rtb-07e7d4ec3f1375ca6) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: <unnamed> (rtb-0ef28ce638540e84a) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-mgmt-az1 (rtb-0eee5939c97efa4e4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-tgw-az2 (rtb-016d95d5808e9bbf5) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-data-az2 (rtb-000195c790a633e47) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-data-az3 (rtb-00e50170ccae7626d) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-mgmt-az2 (rtb-09621ae7c7ba3d852) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-tgw-az1 (rtb-0ca7ddd0d9035b389) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-tgw-az3 (rtb-0ee75094a5c9892d4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-use1-data-az1 (rtb-02734e8fb3ce20530) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.4.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-tgw-az1 (rtb-038a489cf0450c845) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-0b94773d32ad6369b | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-tgw-az3 (rtb-0fae1ce966892e031) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-045e12b4634f99209 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-gwlbe-az3 (rtb-05d6f92dc60058c21) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-data-az3 (rtb-0d704f8fa8af0323c) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-mgmt-az2 (rtb-0f38ffe8ca43a69b6) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-06f582fb83760ad51 | CreateRoute | | 172.16.0.0/12 | tgw-06f582fb83760ad51 | CreateRoute | | 10.0.0.0/8 | tgw-06f582fb83760ad51 | CreateRoute | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-public-az3 (rtb-0cd9e7ab8d2f7441d) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0b46e581f80bc6f48 | CreateRoute | | pl-63a5400a | vpce-04a78f45355d0a523 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-gwlbe-az2 (rtb-08438ea08c40719ee) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-public-az1 (rtb-07570b9770cc42df2) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0b46e581f80bc6f48 | CreateRoute | | pl-63a5400a | vpce-04a78f45355d0a523 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: <unnamed> (rtb-08eadc94948e477f4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-tgw-az2 (rtb-0dd628b462e768da0) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-021971d25af923efa | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-data-az1 (rtb-050773951feba8070) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-data-az2 (rtb-08a60efbe3e867657) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-public-az2 (rtb-0d0ddc98eb5ec241f) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0b46e581f80bc6f48 | CreateRoute | | pl-63a5400a | vpce-04a78f45355d0a523 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-gwlbe-az1 (rtb-0e9b943222cdd3b59) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-mgmt-az1 (rtb-0dfca6838fb46ad87) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-06f582fb83760ad51 | CreateRoute | | 172.16.0.0/12 | tgw-06f582fb83760ad51 | CreateRoute | | 10.0.0.0/8 | tgw-06f582fb83760ad51 | CreateRoute | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-use1-mgmt-az3 (rtb-0a145b986c8ad6006) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.201.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-06f582fb83760ad51 | CreateRoute | | 172.16.0.0/12 | tgw-06f582fb83760ad51 | CreateRoute | | 10.0.0.0/8 | tgw-06f582fb83760ad51 | CreateRoute | | 0.0.0.0/0 | tgw-06f582fb83760ad51 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-data-az3 (rtb-00000639405f588ed) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-data-az2 (rtb-03d32f483551ce73a) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-mgmt-az3 (rtb-063f6851247452e3d) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-mgmt-az1 (rtb-0d9200f9ac56fa654) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-mgmt-az2 (rtb-00b0ed610ae9b5426) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-tgw-az3 (rtb-05ccbd32bb791795c) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-data-az1 (rtb-073fd47c51650f724) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-tgw-az2 (rtb-065544fb1d06e9d22) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: <unnamed> (rtb-01af00f61f711ee5a) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / RT: gbtcloud-transit-ingress-usw2-tgw-az1 (rtb-0d3ab06f1b767a1ff) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.4.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-public-az2 (rtb-080f6ad9a7a9b16b4) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0fe42b1925e490179 | CreateRoute | | pl-68a54001 | vpce-034e58993cbfc09ad | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-data-az2 (rtb-09d5eb639d5191b57) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-mgmt-az1 (rtb-0d3f00818765398b7) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-gwlbe-az2 (rtb-07a36eac2d2effc0f) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: <unnamed> (rtb-04b0af9d13718e879) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-public-az3 (rtb-07695129fc1f7db68) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0fe42b1925e490179 | CreateRoute | | pl-68a54001 | vpce-034e58993cbfc09ad | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-tgw-az3 (rtb-02a47bffbff43ca04) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-0d6010360a464a36b | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-gwlbe-az1 (rtb-0fbc4ebe7f4825d8c) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-data-az1 (rtb-05454afe4c4b7bf09) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-public-az1 (rtb-091fa484a63bd1a1d) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | igw-0fe42b1925e490179 | CreateRoute | | pl-68a54001 | vpce-034e58993cbfc09ad | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-mgmt-az2 (rtb-03ebbdf0f2d83399f) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-data-az3 (rtb-0cd2fe1df261c2112) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-tgw-az2 (rtb-07030a424dfe630c8) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-092a07fbbf24eedea | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-mgmt-az3 (rtb-0bfac5a4517f28b00) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | | 0.0.0.0/0 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-gwlbe-az3 (rtb-05b2f7cb9e4c3b63d) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 192.168.0.0/16 | tgw-062d9465d145ed9e2 | CreateRoute | | 172.16.0.0/12 | tgw-062d9465d145ed9e2 | CreateRoute | | 10.0.0.0/8 | tgw-062d9465d145ed9e2 | CreateRoute | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / RT: gbtcloud-transit-egress-east-west-usw2-tgw-az1 (rtb-0eaddfd6842b09eab) |
| |  |  |  | | --- | --- | --- | | DESTINATION | TARGET | ORIGIN | | 10.228.0.0/22 | local | CreateRouteTable | | 0.0.0.0/0 | vpce-0432038eefe98a907 | CreateRoute | |

# Prefix Lists

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  | | --- | --- | --- | | NAME | ID | CIDRS | | com.amazonaws.eu-west-1.dynamodb | pl-6fa54006 | 52.94.5.0/24 35.71.72.0/22 52.94.26.0/25 52.119.240.0/21 52.94.24.0/23 | | com.amazonaws.eu-west-1.s3 | pl-6da54004 | 18.34.240.0/22 18.34.32.0/20 3.5.64.0/21 3.5.72.0/23 52.92.0.0/17 52.218.0.0/17 | |
| Region: us-east-1 |
| |  |  |  | | --- | --- | --- | | NAME | ID | CIDRS | | com.amazonaws.us-east-1.s3 | pl-63a5400a | 16.182.0.0/16 18.34.0.0/19 52.216.0.0/15 54.231.0.0/16 3.5.0.0/19 18.34.232.0/21 | | com.amazonaws.us-east-1.dynamodb | pl-02cd2c6b | 35.71.70.0/24 3.218.182.0/24 3.218.180.0/23 35.71.68.0/23 52.94.0.0/22 52.119.224.0/20 | |
| Region: us-west-2 |
| |  |  |  | | --- | --- | --- | | NAME | ID | CIDRS | | com.amazonaws.us-west-2.s3 | pl-68a54001 | 3.5.76.0/22 3.5.80.0/21 18.34.48.0/20 18.34.244.0/22 52.92.128.0/17 52.218.128.0/17 | | com.amazonaws.us-west-2.dynamodb | pl-00a54069 | 52.94.28.0/23 52.94.10.0/24 35.71.64.0/22 | |

# Subnets

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.206.0.192/28 | gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ1 | eu-west-1a | rtb-03fe2a41e26fda7cc | acl-0c8fd3f1108116e50 | subnet-047b36d8680df0b08 | 1 | | 10.206.0.48/28 | gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ1 | eu-west-1a | rtb-07c1d78423620f600 | acl-0c8fd3f1108116e50 | subnet-0efb73c4242d840c9 | 1 | | 10.206.0.0/28 | gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ1 | eu-west-1a | rtb-0e36665306abe2a08 | acl-0c8fd3f1108116e50 | subnet-044b170482feebaf7 | 1 | | 10.206.0.144/28 | gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ1 | eu-west-1a | rtb-0e3bd694abe5fedd4 | acl-0c8fd3f1108116e50 | subnet-08deff8f60a566b99 | 0 | | 10.206.0.96/28 | gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ1 | eu-west-1a | rtb-064b343b8c5a6a8b2 | acl-0c8fd3f1108116e50 | subnet-03332dc8bb96207a8 | 0 | | 10.206.0.64/28 | gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ2 | eu-west-1b | rtb-033fc266c592aec05 | acl-0c8fd3f1108116e50 | subnet-0faaa483434284bf2 | 1 | | 10.206.0.160/28 | gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ2 | eu-west-1b | rtb-0cbda1054025672fb | acl-0c8fd3f1108116e50 | subnet-0935957ed69df321a | 0 | | 10.206.0.16/28 | gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ2 | eu-west-1b | rtb-0ddc5998187759fe8 | acl-0c8fd3f1108116e50 | subnet-01172f1cc5eb6e7c8 | 1 | | 10.206.0.208/28 | gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ2 | eu-west-1b | rtb-017e35f2e59206196 | acl-0c8fd3f1108116e50 | subnet-012c022e55482f0e3 | 1 | | 10.206.0.112/28 | gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ2 | eu-west-1b | rtb-081eb9730ab875a17 | acl-0c8fd3f1108116e50 | subnet-0cde0b9864488adb6 | 0 | | 10.206.0.224/28 | gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ3 | eu-west-1c | rtb-0ac72e591abc7ed37 | acl-0c8fd3f1108116e50 | subnet-08babfb693ceba8d7 | 1 | | 10.206.0.32/28 | gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ3 | eu-west-1c | rtb-03352845967b57f01 | acl-0c8fd3f1108116e50 | subnet-0e7b7fda70a4378d7 | 1 | | 10.206.0.80/28 | gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ3 | eu-west-1c | rtb-0f999eb741339a2de | acl-0c8fd3f1108116e50 | subnet-0929ed3d913b63e35 | 1 | | 10.206.0.176/28 | gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ3 | eu-west-1c | rtb-06f34c0fd71f7f82f | acl-0c8fd3f1108116e50 | subnet-0f70fb72038bec455 | 0 | | 10.206.0.128/28 | gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ3 | eu-west-1c | rtb-08ca7f2074ec9d229 | acl-0c8fd3f1108116e50 | subnet-0799fd7349f42ecce | 0 | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.206.4.144/28 | gbtcloud-transit-ingress-euw1-TGWSubnet-AZ1 | eu-west-1a | rtb-09d4fb237eb379200 | acl-0c93ba7c984908a92 | subnet-0137d896dcc0826b1 | 0 | | 10.206.4.192/28 | gbtcloud-transit-ingress-euw1-DataSubnet-AZ1 | eu-west-1a | rtb-0865f8e81a686db9c | acl-0c93ba7c984908a92 | subnet-0b7cc295e657bc900 | 1 | | 10.206.4.48/28 | gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ1 | eu-west-1a | rtb-0d9db8094db8d3d9f | acl-0c93ba7c984908a92 | subnet-041a8830ec6be5eff | 1 | | 10.206.4.64/28 | gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ2 | eu-west-1b | rtb-0b716323014029275 | acl-0c93ba7c984908a92 | subnet-0c50807935eca55ee | 1 | | 10.206.4.160/28 | gbtcloud-transit-ingress-euw1-TGWSubnet-AZ2 | eu-west-1b | rtb-0d4f8906a3285eb73 | acl-0c93ba7c984908a92 | subnet-0ae53d78e331ec645 | 0 | | 10.206.4.208/28 | gbtcloud-transit-ingress-euw1-DataSubnet-AZ2 | eu-west-1b | rtb-0ee9cc74fd1dc13a4 | acl-0c93ba7c984908a92 | subnet-04d20ca271b2037e8 | 1 | | 10.206.4.80/28 | gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ3 | eu-west-1c | rtb-033b68bbf0d4e5449 | acl-0c93ba7c984908a92 | subnet-067c3ec94561daedc | 1 | | 10.206.4.224/28 | gbtcloud-transit-ingress-euw1-DataSubnet-AZ3 | eu-west-1c | rtb-05680d7a934638399 | acl-0c93ba7c984908a92 | subnet-0efe857ac9c1f277c | 1 | | 10.206.4.176/28 | gbtcloud-transit-ingress-euw1-TGWSubnet-AZ3 | eu-west-1c | rtb-073f5d2b17550b9aa | acl-0c93ba7c984908a92 | subnet-0590c8c183554f48a | 0 | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.201.4.48/28 | gbtcloud-transit-ingress-use1-MgmtSubnet-AZ1 | us-east-1a | rtb-0eee5939c97efa4e4 | acl-0acb681cf1682fe21 | subnet-06df68360ca86da15 | 1 | | 10.201.4.144/28 | gbtcloud-transit-ingress-use1-TGWSubnet-AZ1 | us-east-1a | rtb-0ca7ddd0d9035b389 | acl-0acb681cf1682fe21 | subnet-03336e5c9e9b45a17 | 0 | | 10.201.4.192/28 | gbtcloud-transit-ingress-use1-DataSubnet-AZ1 | us-east-1a | rtb-02734e8fb3ce20530 | acl-0acb681cf1682fe21 | subnet-0b43a92182056a059 | 1 | | 10.201.4.208/28 | gbtcloud-transit-ingress-use1-DataSubnet-AZ2 | us-east-1b | rtb-000195c790a633e47 | acl-0acb681cf1682fe21 | subnet-09cd58c7ca6e18f78 | 1 | | 10.201.4.160/28 | gbtcloud-transit-ingress-use1-TGWSubnet-AZ2 | us-east-1b | rtb-016d95d5808e9bbf5 | acl-0acb681cf1682fe21 | subnet-064d41bd7ec4b43ac | 0 | | 10.201.4.64/28 | gbtcloud-transit-ingress-use1-MgmtSubnet-AZ2 | us-east-1b | rtb-09621ae7c7ba3d852 | acl-0acb681cf1682fe21 | subnet-0ebd346130a6a4f21 | 1 | | 10.201.4.224/28 | gbtcloud-transit-ingress-use1-DataSubnet-AZ3 | us-east-1d | rtb-00e50170ccae7626d | acl-0acb681cf1682fe21 | subnet-069dca8181c1d46c7 | 2 | | 10.201.4.176/28 | gbtcloud-transit-ingress-use1-TGWSubnet-AZ3 | us-east-1d | rtb-0ee75094a5c9892d4 | acl-0acb681cf1682fe21 | subnet-09e530aa492b63d2e | 0 | | 10.201.4.80/28 | gbtcloud-transit-ingress-use1-MgmtSubnet-AZ3 | us-east-1d | rtb-07e7d4ec3f1375ca6 | acl-0acb681cf1682fe21 | subnet-07126fcf9b6869e52 | 1 | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.201.0.96/28 | gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ1 | us-east-1a | rtb-0e9b943222cdd3b59 | acl-00299afd85745383e | subnet-0bb8a769ef699414c | 0 | | 10.201.0.144/28 | gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ1 | us-east-1a | rtb-038a489cf0450c845 | acl-00299afd85745383e | subnet-06bee1fc4ef0d8d7c | 0 | | 10.201.0.0/28 | gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ1 | us-east-1a | rtb-07570b9770cc42df2 | acl-00299afd85745383e | subnet-06cdf28668685bb3a | 2 | | 10.201.0.192/28 | gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ1 | us-east-1a | rtb-050773951feba8070 | acl-00299afd85745383e | subnet-08abcdb3032981389 | 3 | | 10.201.0.48/28 | gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ1 | us-east-1a | rtb-0dfca6838fb46ad87 | acl-00299afd85745383e | subnet-0206007c6c5c34387 | 2 | | 10.201.0.208/28 | gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ2 | us-east-1b | rtb-08a60efbe3e867657 | acl-00299afd85745383e | subnet-06d3aae69ad09e76b | 2 | | 10.201.0.64/28 | gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ2 | us-east-1b | rtb-0f38ffe8ca43a69b6 | acl-00299afd85745383e | subnet-0896aa0ebae1ef5e4 | 2 | | 10.201.0.160/28 | gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ2 | us-east-1b | rtb-0dd628b462e768da0 | acl-00299afd85745383e | subnet-0bcbdae9b75a661fd | 0 | | 10.201.0.16/28 | gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ2 | us-east-1b | rtb-0d0ddc98eb5ec241f | acl-00299afd85745383e | subnet-01c1e38462c29aed9 | 2 | | 10.201.0.112/28 | gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ2 | us-east-1b | rtb-08438ea08c40719ee | acl-00299afd85745383e | subnet-0f31d0ef41bc83d8d | 0 | | 10.201.0.176/28 | gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ3 | us-east-1d | rtb-0fae1ce966892e031 | acl-00299afd85745383e | subnet-010846fff1f28cc6d | 0 | | 10.201.0.128/28 | gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ3 | us-east-1d | rtb-05d6f92dc60058c21 | acl-00299afd85745383e | subnet-05eb4245157cd17fe | 0 | | 10.201.0.224/28 | gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ3 | us-east-1d | rtb-0d704f8fa8af0323c | acl-00299afd85745383e | subnet-005c0c6cab91c08f1 | 3 | | 10.201.0.32/28 | gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ3 | us-east-1d | rtb-0cd9e7ab8d2f7441d | acl-00299afd85745383e | subnet-0ac717436d1186181 | 3 | | 10.201.0.80/28 | gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ3 | us-east-1d | rtb-0a145b986c8ad6006 | acl-00299afd85745383e | subnet-027ec1fdb8d160cab | 3 | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.228.4.192/28 | gbtcloud-transit-ingress-usw2-DataSubnet-AZ1 | us-west-2a | rtb-073fd47c51650f724 | acl-077f08622e2633d4f | subnet-0cc312e8737099d62 | 1 | | 10.228.4.144/28 | gbtcloud-transit-ingress-usw2-TGWSubnet-AZ1 | us-west-2a | rtb-0d3ab06f1b767a1ff | acl-077f08622e2633d4f | subnet-08935963a1ec4dd0f | 0 | | 10.228.4.48/28 | gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ1 | us-west-2a | rtb-0d9200f9ac56fa654 | acl-077f08622e2633d4f | subnet-09bcaa5b1386feb2e | 1 | | 10.228.4.208/28 | gbtcloud-transit-ingress-usw2-DataSubnet-AZ2 | us-west-2b | rtb-03d32f483551ce73a | acl-077f08622e2633d4f | subnet-00caacfc0213289c6 | 1 | | 10.228.4.160/28 | gbtcloud-transit-ingress-usw2-TGWSubnet-AZ2 | us-west-2b | rtb-065544fb1d06e9d22 | acl-077f08622e2633d4f | subnet-0edb3719603907493 | 0 | | 10.228.4.64/28 | gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ2 | us-west-2b | rtb-00b0ed610ae9b5426 | acl-077f08622e2633d4f | subnet-0ec8a9d381c3104a8 | 1 | | 10.228.4.224/28 | gbtcloud-transit-ingress-usw2-DataSubnet-AZ3 | us-west-2c | rtb-00000639405f588ed | acl-077f08622e2633d4f | subnet-0cda254219dfbdc12 | 1 | | 10.228.4.80/28 | gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ3 | us-west-2c | rtb-063f6851247452e3d | acl-077f08622e2633d4f | subnet-0fa7f4bef4db50282 | 1 | | 10.228.4.176/28 | gbtcloud-transit-ingress-usw2-TGWSubnet-AZ3 | us-west-2c | rtb-05ccbd32bb791795c | acl-077f08622e2633d4f | subnet-008f3fef0ac09711c | 0 | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | SUBNET | SUBNET NAME | AVAILABILITY ZONE | ROUTE TABLE | NET ACL | ID | INST QTY | | 10.228.0.0/28 | gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ1 | us-west-2a | rtb-091fa484a63bd1a1d | acl-0ce9342bb18c6b9b7 | subnet-08cbba5a6f687cc44 | 1 | | 10.228.0.96/28 | gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ1 | us-west-2a | rtb-0fbc4ebe7f4825d8c | acl-0ce9342bb18c6b9b7 | subnet-0f96f5c6e4813f43b | 0 | | 10.228.0.192/28 | gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ1 | us-west-2a | rtb-05454afe4c4b7bf09 | acl-0ce9342bb18c6b9b7 | subnet-0d73be1ad800b7008 | 1 | | 10.228.0.48/28 | gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ1 | us-west-2a | rtb-0d3f00818765398b7 | acl-0ce9342bb18c6b9b7 | subnet-00a22a642d83879be | 1 | | 10.228.0.144/28 | gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ1 | us-west-2a | rtb-0eaddfd6842b09eab | acl-0ce9342bb18c6b9b7 | subnet-03e3f4e03d83fd384 | 0 | | 10.228.0.160/28 | gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ2 | us-west-2b | rtb-07030a424dfe630c8 | acl-0ce9342bb18c6b9b7 | subnet-0c680b053b98cb89d | 0 | | 10.228.0.112/28 | gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ2 | us-west-2b | rtb-07a36eac2d2effc0f | acl-0ce9342bb18c6b9b7 | subnet-08a09be95ccba364d | 0 | | 10.228.0.64/28 | gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ2 | us-west-2b | rtb-03ebbdf0f2d83399f | acl-0ce9342bb18c6b9b7 | subnet-001e537abca8620c8 | 1 | | 10.228.0.16/28 | gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ2 | us-west-2b | rtb-080f6ad9a7a9b16b4 | acl-0ce9342bb18c6b9b7 | subnet-06ff9bd4330a6e906 | 1 | | 10.228.0.208/28 | gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ2 | us-west-2b | rtb-09d5eb639d5191b57 | acl-0ce9342bb18c6b9b7 | subnet-0334b4095a7630a4f | 1 | | 10.228.0.80/28 | gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ3 | us-west-2c | rtb-0bfac5a4517f28b00 | acl-0ce9342bb18c6b9b7 | subnet-0d7a07d117c0d5af6 | 1 | | 10.228.0.128/28 | gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ3 | us-west-2c | rtb-05b2f7cb9e4c3b63d | acl-0ce9342bb18c6b9b7 | subnet-0becadb33514fcb5f | 0 | | 10.228.0.224/28 | gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ3 | us-west-2c | rtb-0cd2fe1df261c2112 | acl-0ce9342bb18c6b9b7 | subnet-0038de275ab5144d8 | 1 | | 10.228.0.176/28 | gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ3 | us-west-2c | rtb-02a47bffbff43ca04 | acl-0ce9342bb18c6b9b7 | subnet-082c777b037dd663b | 0 | | 10.228.0.32/28 | gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ3 | us-west-2c | rtb-07695129fc1f7db68 | acl-0ce9342bb18c6b9b7 | subnet-0b1b9f9bc74795934 | 1 | |

# Network ACLs

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-0c8fd3f1108116e50 | yes | subnet-0935957ed69df321a subnet-0f70fb72038bec455 subnet-0929ed3d913b63e35 subnet-0faaa483434284bf2 subnet-0799fd7349f42ecce subnet-012c022e55482f0e3 subnet-01172f1cc5eb6e7c8 subnet-0e7b7fda70a4378d7 subnet-08babfb693ceba8d7 subnet-047b36d8680df0b08 subnet-03332dc8bb96207a8 subnet-0efb73c4242d840c9 subnet-0cde0b9864488adb6 subnet-044b170482feebaf7 subnet-08deff8f60a566b99 | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-0c93ba7c984908a92 | yes | subnet-0137d896dcc0826b1 subnet-041a8830ec6be5eff subnet-0590c8c183554f48a subnet-04d20ca271b2037e8 subnet-0efe857ac9c1f277c subnet-0b7cc295e657bc900 subnet-0c50807935eca55ee subnet-067c3ec94561daedc subnet-0ae53d78e331ec645 | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-0acb681cf1682fe21 | yes | subnet-03336e5c9e9b45a17 subnet-09e530aa492b63d2e subnet-06df68360ca86da15 subnet-09cd58c7ca6e18f78 subnet-0ebd346130a6a4f21 subnet-064d41bd7ec4b43ac subnet-0b43a92182056a059 subnet-07126fcf9b6869e52 subnet-069dca8181c1d46c7 | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-00299afd85745383e | yes | subnet-06cdf28668685bb3a subnet-05eb4245157cd17fe subnet-0f31d0ef41bc83d8d subnet-01c1e38462c29aed9 subnet-0ac717436d1186181 subnet-0bb8a769ef699414c subnet-08abcdb3032981389 subnet-010846fff1f28cc6d subnet-0896aa0ebae1ef5e4 subnet-06bee1fc4ef0d8d7c subnet-0bcbdae9b75a661fd subnet-027ec1fdb8d160cab subnet-0206007c6c5c34387 subnet-005c0c6cab91c08f1 subnet-06d3aae69ad09e76b | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-077f08622e2633d4f | yes | subnet-09bcaa5b1386feb2e subnet-0cc312e8737099d62 subnet-0edb3719603907493 subnet-00caacfc0213289c6 subnet-0ec8a9d381c3104a8 subnet-08935963a1ec4dd0f subnet-008f3fef0ac09711c subnet-0fa7f4bef4db50282 subnet-0cda254219dfbdc12 | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  | | --- | --- | --- | --- | | ACL NAME | ACL ID | IS DEFAULT | SUBNETS | |  | acl-0ce9342bb18c6b9b7 | yes | subnet-0f96f5c6e4813f43b subnet-00a22a642d83879be subnet-0d73be1ad800b7008 subnet-0c680b053b98cb89d subnet-08cbba5a6f687cc44 subnet-03e3f4e03d83fd384 subnet-08a09be95ccba364d subnet-0334b4095a7630a4f subnet-06ff9bd4330a6e906 subnet-082c777b037dd663b subnet-0038de275ab5144d8 subnet-0becadb33514fcb5f subnet-0b1b9f9bc74795934 subnet-0d7a07d117c0d5af6 subnet-001e537abca8620c8 | |

# Network ACL – Inbound Entries

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-0c8fd3f1108116e50) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-0c93ba7c984908a92) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-0acb681cf1682fe21) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-00299afd85745383e) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-077f08622e2633d4f) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-0ce9342bb18c6b9b7) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |

# Network ACL – Outbound Entries

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-0c8fd3f1108116e50) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-0c93ba7c984908a92) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-0acb681cf1682fe21) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-00299afd85745383e) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / ACL: <unnamed> (acl-077f08622e2633d4f) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / ACL: <unnamed> (acl-0ce9342bb18c6b9b7) |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | RULE NUMBER | PROTOCOL | PORT RANGE | SOURCE | ACTION | | 100 | All Traffic | All | 0.0.0.0/0 | allow | | 32767 | All Traffic | All | 0.0.0.0/0 | deny | |

# Security Groups

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | vpc-egress-east-west-VMSeries-Egress | vpc-egress-east-west-VMSeriesEgressSecurityGroup-8ITDFVG3309X | sg-052b322624c487107 | VM-Series Egress Security Group | 0/1 | | vpc-egress-east-west-VMSeries-Management | vpc-egress-east-west-VMSeriesManagementSecurityGroup-LH94W695MHCE | sg-009d2a9f849023fad | VM-Series Management Security Group | 3/1 | | sg-default-DO-NOT-USE | default | sg-0f4581e6f0e2548f5 | default VPC security group | 0/0 | | vpc-egress-east-west-VMSeries-Data | vpc-egress-east-west-VMSeriesDataSecurityGroup-NLSSGMW30Z2B | sg-0ece74c8634d2bcbe | VM-Series Data Security Group | 1/1 | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | vpc-ingress-VMSeries-Data | vpc-ingress-VMSeriesDataSecurityGroup-YM5JZ47ZUIK8 | sg-080992c081971b7df | VM-Series Data Security Group | 1/1 | | vpc-ingress-VMSeries-Management | vpc-ingress-VMSeriesManagementSecurityGroup-1TSGC9GM8FAA6 | sg-0410a18e5adea3b16 | VM-Series Management Security Group | 3/1 | | sg-default-DO-NOT-USE | default | sg-006f3ebb8a6b9d4c3 | default VPC security group | 0/0 | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | sg-default-DO-NOT-USE | default | sg-0309ea6c436145838 | default VPC security group | 0/0 | | vpc-ingress-VMSeries-Data | vpc-ingress-VMSeriesDataSecurityGroup-KG4SHQ7DR31I | sg-05771702e0bbb1754 | VM-Series Data Security Group | 1/1 | |  | Security Group for SSH Troubleshooting | sg-03d5a5b986a45a183 | Security Group for SSH Troubleshooting | 1/1 | | vpc-ingress-VMSeries-Management | vpc-ingress-VMSeriesManagementSecurityGroup-WPGR6YG0LO8I | sg-01dee5b2f04991bb1 | VM-Series Management Security Group | 8/1 | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | sg-default-DO-NOT-USE | default | sg-057819166143a3762 | default VPC security group | 0/0 | | vpc-egress-east-west-VMSeries-Egress | vpc-egress-east-west-VMSeriesEgressSecurityGroup-U3O9WXEQ4YNR | sg-0553ef4f38bf13091 | VM-Series Egress Security Group | 0/1 | | vpc-egress-east-west-VMSeries-Data | vpc-egress-east-west-VMSeriesDataSecurityGroup-OLINT5AU37C7 | sg-0745b4634b4d34ee9 | VM-Series Data Security Group | 1/1 | |  | sgec2-liveaction-Transit-01-use1 | sg-0dbd0cb854378bdc6 | sgec2-liveaction-Transit-01-use1 | 13/1 | |  | sgec2-Transit-common-sg-01-use1 | sg-0316292a888ef84bf | sgec2-Transit-common-sg-01-use1 | 3/1 | | vpc-egress-east-west-VMSeries-Management | vpc-egress-east-west-VMSeriesManagementSecurityGroup-188NBW9WNNIP2 | sg-08582a4436c53e22e | VM-Series Management Security Group | 10/1 | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | sg-default-DO-NOT-USE | default | sg-0ffeb39191f60ef63 | default VPC security group | 0/0 | | vpc-ingress-VMSeries-Management | vpc-ingress-VMSeriesManagementSecurityGroup-12JXPUWBPQVLQ | sg-083652d7e289a206a | VM-Series Management Security Group | 3/1 | | vpc-ingress-VMSeries-Data | vpc-ingress-VMSeriesDataSecurityGroup-1FBI8C886FBY9 | sg-08801f2668550b9a6 | VM-Series Data Security Group | 1/1 | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | SG NAME (TAG) | SG NAME | SG ID | DESCRIPTION | IN/OUT RULE COUNT | | sg-default-DO-NOT-USE | default | sg-0bb6f5ca692dcfbbb | default VPC security group | 0/0 | | vpc-egress-east-west-VMSeries-Management | vpc-egress-east-west-VMSeriesManagementSecurityGroup-1AI4JVH6HET7T | sg-02cede6aee227f247 | VM-Series Management Security Group | 3/1 | | vpc-egress-east-west-VMSeries-Data | vpc-egress-east-west-VMSeriesDataSecurityGroup-Y6MAQUSQPUDU | sg-0526cb6fbaec4c1b0 | VM-Series Data Security Group | 1/1 | | vpc-egress-east-west-VMSeries-Egress | vpc-egress-east-west-VMSeriesEgressSecurityGroup-KWO7GMLMIFHS | sg-0e8c49685c1dca9bc | VM-Series Egress Security Group | 0/1 | |

# Security Group – Inbound Entries

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-052b322624c487107) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-009d2a9f849023fad) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 443 | 10.156.195.27/32 |  | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | tcp | 443 | 10.194.45.44/32 |  | | icmp | -1 | 10.0.0.0/8 |  | | icmp | -1 | 10.194.45.44/32 |  | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0f4581e6f0e2548f5) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0ece74c8634d2bcbe) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-080992c081971b7df) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-0410a18e5adea3b16) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | tcp | 443 | 10.156.195.27/32 |  | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | tcp | 443 | 10.194.45.44/32 |  | | icmp | -1 | 10.0.0.0/8 |  | | icmp | -1 | 10.194.45.44/32 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-006f3ebb8a6b9d4c3) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0309ea6c436145838) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-05771702e0bbb1754) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 10.201.4.224/28 | data interface subnet for GWLB health probes and GENEVE | | All | All | 10.201.4.192/28 | data interface subnet for GWLB health probes and GENEVE | | All | All | 10.201.4.208/28 | data interface subnet for GWLB health probes and GENEVE | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: <unnamed> (sg-03d5a5b986a45a183) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | tcp | 22 | 10.0.0.0/8 |  | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-01dee5b2f04991bb1) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | udp | 161 | 10.156.241.220/32 | WTC Live NX | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | tcp | 6367 | 10.156.241.220/32 | WTC Live NX | | udp | 2055 | 10.156.241.220/32 | WTC Live NX | | tcp | 8443 | 10.156.241.220/32 | WTC Live NX | | udp | 4789 | 10.156.241.220/32 | WTC Live NX | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.156.195.27/32 | WTC Live NX | | tcp | 443 | 10.194.45.44/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | icmp | -1 | 10.194.45.44/32 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-057819166143a3762) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-0553ef4f38bf13091) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0745b4634b4d34ee9) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: <unnamed> (sg-0dbd0cb854378bdc6) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | udp | 161 | 10.0.0.0/8 |  | | tcp | 80 | 10.0.0.0/8 |  | | tcp | 8092 | 10.0.0.0/8 |  | | tcp | 22 | 10.0.0.0/8 |  | | tcp | 9443 | 10.0.0.0/8 |  | | tcp | 161 | 10.0.0.0/8 |  | | tcp | 6367 | 10.0.0.0/8 |  | | udp | 2055 | 10.0.0.0/8 |  | | tcp | 8443 | 10.0.0.0/8 |  | | tcp | 7000 | 10.0.0.0/8 |  | | udp | 4789 | 10.0.0.0/8 |  | | tcp | 443 | 10.0.0.0/8 |  | | tcp | 8093 | 10.0.0.0/8 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: <unnamed> (sg-0316292a888ef84bf) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 10.201.0.0/20 |  | | All | All | 192.168.0.0/16 |  | | All | All | 10.192.0.0/13 |  | | All | All | 172.16.0.0/12 |  | | All | All | 10.201.17.57/32 |  | | All | All | 10.202.0.0/15 |  | | All | All | 10.204.0.0/14 |  | | All | All | 10.200.0.0/16 |  | | All | All | 10.0.0.0/9 |  | | All | All | 10.128.0.0/10 |  | | All | All | 10.201.24.0/21 |  | | All | All | 10.201.64.0/18 |  | | All | All | 10.201.128.0/17 |  | | All | All | 10.201.32.0/19 |  | | All | All | 10.208.0.0/12 |  | | All | All | 10.201.20.0/22 |  | | All | All | 10.224.0.0/11 |  | | tcp | 2144 | 10.201.18.41/32 |  | | tcp | 2144 | 10.201.16.65/32 |  | | tcp | 2144 | 10.201.17.104/32 |  | | tcp | 18080 | 10.201.17.0/24 |  | | tcp | 18080 | 10.201.18.0/24 |  | | tcp | 18080 | 10.201.16.0/24 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-08582a4436c53e22e) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | udp | 161 | 10.201.16.134/32 | AWS Live NX | | tcp | 5007 | 10.157.21.57/32 |  | | tcp | 5007 | 10.193.13.10/32 |  | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 6367 | 10.201.16.134/32 | AWS Live NX | | udp | 2055 | 10.201.16.134/32 | AWS Live NX | | tcp | 8443 | 10.201.16.134/32 | AWS Live NX | | udp | 4789 | 10.201.16.134/32 | AWS Live NX | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.156.195.27/32 |  | | tcp | 443 | 10.194.45.44/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | icmp | -1 | 10.194.45.44/32 |  | | icmp | 8--1 | 10.193.13.10/32 |  | | icmp | 8--1 | 10.157.21.57/32 |  | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0ffeb39191f60ef63) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-083652d7e289a206a) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.156.195.27/32 |  | | tcp | 443 | 10.194.45.44/32 |  | | icmp | -1 | 10.194.45.44/32 |  | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-08801f2668550b9a6) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0bb6f5ca692dcfbbb) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-02cede6aee227f247) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | tcp | 22 | 10.194.68.10/32 |  | | tcp | 22 | 10.156.195.27/32 |  | | tcp | 22 | 10.193.13.10/32 |  | | tcp | 22 | 10.194.45.44/32 |  | | icmp | -1 | 10.194.45.44/32 |  | | tcp | 443 | 10.194.68.10/32 |  | | tcp | 443 | 10.193.13.10/32 |  | | tcp | 443 | 10.156.195.27/32 |  | | tcp | 443 | 10.194.45.44/32 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0526cb6fbaec4c1b0) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-0e8c49685c1dca9bc) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |

# Security Group – Outbound Entries

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-052b322624c487107) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-009d2a9f849023fad) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0f4581e6f0e2548f5) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0ece74c8634d2bcbe) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-080992c081971b7df) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-0410a18e5adea3b16) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-006f3ebb8a6b9d4c3) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0309ea6c436145838) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-05771702e0bbb1754) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: <unnamed> (sg-03d5a5b986a45a183) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-01dee5b2f04991bb1) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-057819166143a3762) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-0553ef4f38bf13091) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0745b4634b4d34ee9) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: <unnamed> (sg-0dbd0cb854378bdc6) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: <unnamed> (sg-0316292a888ef84bf) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-08582a4436c53e22e) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0ffeb39191f60ef63) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Management (sg-083652d7e289a206a) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC / SG: vpc-ingress-VMSeries-Data (sg-08801f2668550b9a6) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: sg-default-DO-NOT-USE (sg-0bb6f5ca692dcfbbb) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Management (sg-02cede6aee227f247) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Data (sg-0526cb6fbaec4c1b0) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC / SG: vpc-egress-east-west-VMSeries-Egress (sg-0e8c49685c1dca9bc) |
| |  |  |  |  | | --- | --- | --- | --- | | PROTOCOL | PORT RANGE | SOURCE | DESCRIPTION | | All | All | 0.0.0.0/0 |  | |

# Internet Gateways

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  | | --- | --- | --- | | VPC | IGW NAME | ID | | vpc-egress-east-west-TransitVPC | vpc-egress-east-west-TransitVPC-IGW | igw-01a6711f8ce1612df | | vpc-ingress-TransitVPC | vpc-ingress-TransitVPC-IGW | igw-0e0d3e524d1153532 | |
| Region: us-east-1 |
| |  |  |  | | --- | --- | --- | | VPC | IGW NAME | ID | | vpc-ingress-TransitVPC | vpc-ingress-TransitVPC-IGW | igw-0b2fda9ed7d24ee87 | | vpc-egress-east-west-TransitVPC | vpc-egress-east-west-TransitVPC-IGW | igw-0b46e581f80bc6f48 | |
| Region: us-west-2 |
| |  |  |  | | --- | --- | --- | | VPC | IGW NAME | ID | | vpc-ingress-TransitVPC | vpc-ingress-TransitVPC-IGW | igw-0414e44b0ac8b10c6 | | vpc-egress-east-west-TransitVPC | vpc-egress-east-west-TransitVPC-IGW | igw-0fe42b1925e490179 | |

# Egress-Only Internet Gateways

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  | | --- | --- | --- | | VPC | EIGW NAME | ID | |
| Region: us-east-1 |
| |  |  |  | | --- | --- | --- | | VPC | EIGW NAME | ID | |
| Region: us-west-2 |
| |  |  |  | | --- | --- | --- | | VPC | EIGW NAME | ID | |

# NAT Gateways

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | VPC | NGW NAME | ID | SUBNET | TYPE | |
| Region: us-east-1 |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | VPC | NGW NAME | ID | SUBNET | TYPE | |
| Region: us-west-2 |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | VPC | NGW NAME | ID | SUBNET | TYPE | |

# Endpoint Services

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.eu-west-1.vpce-svc-0016b276173cf67bb | | | | | | | NAME | ingress | ID | vpce-svc-0016b276173cf67bb | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | eu-west-1a eu-west-1b eu-west-1c | | | |
|  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.eu-west-1.vpce-svc-066c38b11701cc071 | | | | | | | NAME | EEW | ID | vpce-svc-066c38b11701cc071 | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | eu-west-1a eu-west-1b eu-west-1c | | | |
| Region: us-east-1 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.us-east-1.vpce-svc-09df5f9ce8a3dfc11 | | | | | | | NAME | EEW | ID | vpce-svc-09df5f9ce8a3dfc11 | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | us-east-1a us-east-1b us-east-1d | | | |
|  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.us-east-1.vpce-svc-0e943307262036cd0 | | | | | | | NAME | ingress | ID | vpce-svc-0e943307262036cd0 | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | us-east-1a us-east-1b us-east-1d | | | |
| Region: us-west-2 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.us-west-2.vpce-svc-007721d5f7a74f1b3 | | | | | | | NAME | <unnamed> | ID | vpce-svc-007721d5f7a74f1b3 | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | us-west-2a us-west-2b us-west-2c | | | |
|  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | ENDPOINT SERVICE NAME: com.amazonaws.vpce.us-west-2.vpce-svc-04c938a4bc78e572a | | | | | | | NAME | <unnamed> | ID | vpce-svc-04c938a4bc78e572a | | | | TYPE | GatewayLoadBalancer | AVAILABILITY ZONES | us-west-2a us-west-2b us-west-2c | | | |

# Endpoints

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | NAME | ID | TYPE | ENI | SUBNETS | SVC NAME | |  | vpce-02050004a100a4b5e | Gateway |  |  | com.amazonaws.eu-west-1.s3 | |  | vpce-001d9d5aad8465874 | GatewayLoadBalancer | eni-05b4c9aa1f2807658 | subnet-03332dc8bb96207a8(gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ1) | com.amazonaws.vpce.eu-west-1.vpce-svc-066c38b11701cc071 | |  | vpce-07d638db429bebe5a | GatewayLoadBalancer | eni-0a421c0877b21174e | subnet-0799fd7349f42ecce(gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ3) | com.amazonaws.vpce.eu-west-1.vpce-svc-066c38b11701cc071 | |  | vpce-024f07b53c9e97eb0 | GatewayLoadBalancer | eni-0c1abc5e2ef0d967b | subnet-0cde0b9864488adb6(gbtcloud-transit-egress-east-west-euw1-GWLBESubnet-AZ2) | com.amazonaws.vpce.eu-west-1.vpce-svc-066c38b11701cc071 | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| No Endpoints present |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| No Endpoints present |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | NAME | ID | TYPE | ENI | SUBNETS | SVC NAME | |  | vpce-04a78f45355d0a523 | Gateway |  |  | com.amazonaws.us-east-1.s3 | | gbtcloud-transit-egress-east-west-use1-GWLBE-AZ1 | vpce-0b94773d32ad6369b | GatewayLoadBalancer | eni-0dc74b23ce7c667b4 | subnet-0bb8a769ef699414c(gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ1) | com.amazonaws.vpce.us-east-1.vpce-svc-09df5f9ce8a3dfc11 | | gbtcloud-transit-egress-east-west-use1-GWLBE-AZ3 | vpce-045e12b4634f99209 | GatewayLoadBalancer | eni-0e088afcf0158fe99 | subnet-05eb4245157cd17fe(gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ3) | com.amazonaws.vpce.us-east-1.vpce-svc-09df5f9ce8a3dfc11 | | gbtcloud-transit-egress-east-west-use1-GWLBE-AZ2 | vpce-021971d25af923efa | GatewayLoadBalancer | eni-012924876256c580b | subnet-0f31d0ef41bc83d8d(gbtcloud-transit-egress-east-west-use1-GWLBESubnet-AZ2) | com.amazonaws.vpce.us-east-1.vpce-svc-09df5f9ce8a3dfc11 | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| No Endpoints present |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | NAME | ID | TYPE | ENI | SUBNETS | SVC NAME | |  | vpce-034e58993cbfc09ad | Gateway |  |  | com.amazonaws.us-west-2.s3 | |  | vpce-0d6010360a464a36b | GatewayLoadBalancer | eni-09be6cf9aed7a0e70 | subnet-0becadb33514fcb5f(gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ3) | com.amazonaws.vpce.us-west-2.vpce-svc-007721d5f7a74f1b3 | |  | vpce-092a07fbbf24eedea | GatewayLoadBalancer | eni-06b33fdb9509e3858 | subnet-08a09be95ccba364d(gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ2) | com.amazonaws.vpce.us-west-2.vpce-svc-007721d5f7a74f1b3 | |  | vpce-0432038eefe98a907 | GatewayLoadBalancer | eni-02e92f9e0626e45c4 | subnet-0f96f5c6e4813f43b(gbtcloud-transit-egress-east-west-usw2-GWLBESubnet-AZ1) | com.amazonaws.vpce.us-west-2.vpce-svc-007721d5f7a74f1b3 | |

# Peering Connections

|  |  |  |  |
| --- | --- | --- | --- |
| No VPC Peerings | | | |

# Transit Gateways

**NOTE:** If the Owner ID is in red, the TGW has been shared from a different account (the owner ID does not match the current account ID).

|  |
| --- |
| Region: eu-west-1 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TRANSIT GATEWAY | | | | | | | TGW NAME |  | | ID | tgw-0ad502a1c2efd4cf8 | | | BGP ASN | 64804 | | OWNER ID | 800999935349 | | | ATTACHMENTS | | | | | | | ATTACHMENT NAME | ATTACHMENT ID | TYPE | RESOURCE ID | ROUTE TABLE ASSOC | SUBNETS | | vpc-egress-east-west-TransitVPC | tgw-attach-00518f0d101e9db77 | vpc (Appliance Mode Enabled) | vpc-02eba02cbd3357bd7 | tgw-rtb-0df25c86fcf1cb0a0 | subnet-0f70fb72038bec455(gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ3) subnet-0935957ed69df321a(gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ2) subnet-08deff8f60a566b99(gbtcloud-transit-egress-east-west-euw1-TGWSubnet-AZ1) | | vpc-ingress-TransitVPC | tgw-attach-0ee6c1a9ba7ba579b | vpc (Appliance Mode Enabled) | vpc-0474c0100ce5e4d3f | tgw-rtb-0df25c86fcf1cb0a0 | subnet-0137d896dcc0826b1(gbtcloud-transit-ingress-euw1-TGWSubnet-AZ1) subnet-0ae53d78e331ec645(gbtcloud-transit-ingress-euw1-TGWSubnet-AZ2) subnet-0590c8c183554f48a(gbtcloud-transit-ingress-euw1-TGWSubnet-AZ3) | | ROUTE TABLES | | | | | | | ROUTE TABLE NAME | | | ROUTE TABLE ID | | | |
| Region: us-east-1 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TRANSIT GATEWAY | | | | | | | TGW NAME |  | | ID | tgw-06f582fb83760ad51 | | | BGP ASN | 64803 | | OWNER ID | 800999935349 | | | ATTACHMENTS | | | | | | | ATTACHMENT NAME | ATTACHMENT ID | TYPE | RESOURCE ID | ROUTE TABLE ASSOC | SUBNETS | | vpc-ingress-TransitVPC | tgw-attach-034763d1bf8d61f8c | vpc (Appliance Mode Enabled) | vpc-09ce0acd298aa0180 | tgw-rtb-0481124cbd523d209 | subnet-09e530aa492b63d2e(gbtcloud-transit-ingress-use1-TGWSubnet-AZ3) subnet-064d41bd7ec4b43ac(gbtcloud-transit-ingress-use1-TGWSubnet-AZ2) subnet-03336e5c9e9b45a17(gbtcloud-transit-ingress-use1-TGWSubnet-AZ1) | | vpc-egress-east-west-TransitVPC | tgw-attach-05307c7b3854a1b91 | vpc (Appliance Mode Enabled) | vpc-00a0fc500fad24c91 | tgw-rtb-0481124cbd523d209 | subnet-06bee1fc4ef0d8d7c(gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ1) subnet-010846fff1f28cc6d(gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ3) subnet-0bcbdae9b75a661fd(gbtcloud-transit-egress-east-west-use1-TGWSubnet-AZ2) | | ROUTE TABLES | | | | | | | ROUTE TABLE NAME | | | ROUTE TABLE ID | | | |
| Region: us-west-2 |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TRANSIT GATEWAY | | | | | | | TGW NAME |  | | ID | tgw-062d9465d145ed9e2 | | | BGP ASN | 64805 | | OWNER ID | 800999935349 | | | ATTACHMENTS | | | | | | | ATTACHMENT NAME | ATTACHMENT ID | TYPE | RESOURCE ID | ROUTE TABLE ASSOC | SUBNETS | |  | tgw-attach-068f46c38e670470b | vpc (Appliance Mode Enabled) | vpc-02745e1fd5db35884 | tgw-rtb-0ab0b80655c808f70 | subnet-0edb3719603907493(gbtcloud-transit-ingress-usw2-TGWSubnet-AZ2) subnet-008f3fef0ac09711c(gbtcloud-transit-ingress-usw2-TGWSubnet-AZ3) subnet-08935963a1ec4dd0f(gbtcloud-transit-ingress-usw2-TGWSubnet-AZ1) | |  | tgw-attach-09d8818363a060955 | vpc (Appliance Mode Enabled) | vpc-06b2af15774b0380c | tgw-rtb-0ab0b80655c808f70 | subnet-0c680b053b98cb89d(gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ2) subnet-082c777b037dd663b(gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ3) subnet-03e3f4e03d83fd384(gbtcloud-transit-egress-east-west-usw2-TGWSubnet-AZ1) | | ROUTE TABLES | | | | | | | ROUTE TABLE NAME | | | ROUTE TABLE ID | | | |

# Transit Gateway Routes

|  |
| --- |
| No Transit Gateway Routes Present |

# VPN – Customer Gateways

|  |
| --- |
| No Customer Gateways attached to transit gateways present |

# VPN – Site-to-Site Connections (Connected to Transit Gateways)

|  |
| --- |
| No VPN Transit Gateway Connections present |

# VPN – Virtual Private Gateways

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| No VPN Gateways configured |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| No VPN Gateways configured |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| No VPN Gateways configured |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| No VPN Gateways configured |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| No VPN Gateways configured |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| No VPN Gateways configured |

# Direct Connect Gateways

|  |
| --- |
| No Direct Connect Gateways present |

# Load Balancers

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:eu-west-1:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/da8ee669798056e1 | | | | | | | NAME | vpc-egress-east-west-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | eu-west-1a | | subnet-047b36d8680df0b08(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ1) | | <none> | | | eu-west-1c | | subnet-08babfb693ceba8d7(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ3) | | <none> | | | eu-west-1b | | subnet-012c022e55482f0e3(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ2) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-egress-east-west-VMSeries | arn:aws:elasticloadbalancing:eu-west-1:195750747780:listener/gwy/vpc-egress-east-west-GWLB/da8ee669798056e1/be53c9868b3aa4e9 | | | | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:eu-west-1:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/27e08330eaaf0383 | | | | | | | NAME | vpc-ingress-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | eu-west-1b | | subnet-04d20ca271b2037e8(gbtcloud-transit-ingress-euw1-DataSubnet-AZ2) | | <none> | | | eu-west-1a | | subnet-0b7cc295e657bc900(gbtcloud-transit-ingress-euw1-DataSubnet-AZ1) | | <none> | | | eu-west-1c | | subnet-0efe857ac9c1f277c(gbtcloud-transit-ingress-euw1-DataSubnet-AZ3) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-ingress-VMSeries | arn:aws:elasticloadbalancing:eu-west-1:195750747780:listener/gwy/vpc-ingress-GWLB/27e08330eaaf0383/f4feefbcd34eeb2e | | | | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:us-east-1:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/6995c69d4cb57862 | | | | | | | NAME | vpc-ingress-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | us-east-1b | | subnet-09cd58c7ca6e18f78(gbtcloud-transit-ingress-use1-DataSubnet-AZ2) | | <none> | | | us-east-1d | | subnet-069dca8181c1d46c7(gbtcloud-transit-ingress-use1-DataSubnet-AZ3) | | <none> | | | us-east-1a | | subnet-0b43a92182056a059(gbtcloud-transit-ingress-use1-DataSubnet-AZ1) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-ingress-VMSeries | arn:aws:elasticloadbalancing:us-east-1:195750747780:listener/gwy/vpc-ingress-GWLB/6995c69d4cb57862/234327f6b03a8c2b | | | | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:us-east-1:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/a370220c9b452046 | | | | | | | NAME | vpc-egress-east-west-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | us-east-1b | | subnet-06d3aae69ad09e76b(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ2) | | <none> | | | us-east-1a | | subnet-08abcdb3032981389(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ1) | | <none> | | | us-east-1d | | subnet-005c0c6cab91c08f1(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ3) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-egress-east-west-VMSeries | arn:aws:elasticloadbalancing:us-east-1:195750747780:listener/gwy/vpc-egress-east-west-GWLB/a370220c9b452046/ea4e9d0f4a4b2ff5 | | | | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:us-west-2:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/31c5da4241bb66a1 | | | | | | | NAME | vpc-ingress-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | us-west-2a | | subnet-0cc312e8737099d62(gbtcloud-transit-ingress-usw2-DataSubnet-AZ1) | | <none> | | | us-west-2b | | subnet-00caacfc0213289c6(gbtcloud-transit-ingress-usw2-DataSubnet-AZ2) | | <none> | | | us-west-2c | | subnet-0cda254219dfbdc12(gbtcloud-transit-ingress-usw2-DataSubnet-AZ3) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-ingress-VMSeries | arn:aws:elasticloadbalancing:us-west-2:195750747780:listener/gwy/vpc-ingress-GWLB/31c5da4241bb66a1/ddca48bae194910d | | | | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | LOAD BALANCER ARN: arn:aws:elasticloadbalancing:us-west-2:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/0b613a42d8050581 | | | | | | | NAME | vpc-egress-east-west-GWLB | TYPE | gateway | STATE | active | | NETWORK MAPPINGS | | | | | | | AVAILABILITY ZONE | | SUBNET | | ADDRESSES | | | us-west-2a | | subnet-0d73be1ad800b7008(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ1) | | <none> | | | us-west-2b | | subnet-0334b4095a7630a4f(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ2) | | <none> | | | us-west-2c | | subnet-0038de275ab5144d8(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ3) | | <none> | | | LISTENERS | | | | | | | PROTOCOL:PORT | FORWARD GROUP | LISTENER ARN | | | | | GENEVE:6081 | vpc-egress-east-west-VMSeries | arn:aws:elasticloadbalancing:us-west-2:195750747780:listener/gwy/vpc-egress-east-west-GWLB/0b613a42d8050581/6717808fe26d330d | | | | |

# Load Balancer Target Groups

|  |
| --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:eu-west-1:195750747780:targetgroup/vpc-egress-east-west-VMSeries/009897512e84aab72c | | | | | | | NAME | vpc-egress-east-west-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:eu-west-1:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/da8ee669798056e1 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 3 | 3 | 5 | 10 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-09e100fc017b51e6f | 6081 | healthy | --- | --- | | | i-0bb50fb55ec372473 | 6081 | healthy | --- | --- | | | i-0a9d430a70bb92221 | 6081 | healthy | --- | --- | | |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:eu-west-1:195750747780:targetgroup/vpc-ingress-VMSeries/004bee91cf5a0f05ea | | | | | | | NAME | vpc-ingress-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:eu-west-1:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/27e08330eaaf0383 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 3 | 3 | 5 | 10 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-010b766c694091022 | 6081 | healthy | --- | --- | | | i-0e2f2015210a7a043 | 6081 | healthy | --- | --- | | | i-065a1e9a62fc6c8fb | 6081 | healthy | --- | --- | | |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:us-east-1:195750747780:targetgroup/vpc-ingress-VMSeries/00b0e5eae5d5667df1 | | | | | | | NAME | vpc-ingress-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:us-east-1:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/6995c69d4cb57862 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 3 | 3 | 2 | 5 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-0319a9685c5d55130 | 6081 | healthy | --- | --- | | | i-0f0b34371a4e321c6 | 6081 | healthy | --- | --- | | | i-090c6188b0f4c8526 | 6081 | healthy | --- | --- | | |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:us-east-1:195750747780:targetgroup/vpc-egress-east-west-VMSeries/007dc1fb73eae6eaac | | | | | | | NAME | vpc-egress-east-west-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:us-east-1:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/a370220c9b452046 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 4 | 4 | 10 | 20 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-071017ef5eeb4c869 | 6081 | healthy | --- | --- | | | i-04df721cb262df221 | 6081 | healthy | --- | --- | | | i-08db73a64101064d9 | 6081 | healthy | --- | --- | | |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:us-west-2:195750747780:targetgroup/vpc-ingress-VMSeries/007ce06067a77441a9 | | | | | | | NAME | vpc-ingress-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:us-west-2:195750747780:loadbalancer/gwy/vpc-ingress-GWLB/31c5da4241bb66a1 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 3 | 3 | 5 | 10 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-04dd921823ef6b565 | 6081 | healthy | --- | --- | | | i-056c44368214abe8f | 6081 | healthy | --- | --- | | | i-020d853d4a8d15f9e | 6081 | healthy | --- | --- | | |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | TARGET GROUP ARN: arn:aws:elasticloadbalancing:us-west-2:195750747780:targetgroup/vpc-egress-east-west-VMSeries/003ffb7c8622cc1636 | | | | | | | NAME | vpc-egress-east-west-VMSeries | PROTOCOL:PORT | GENEVE:6081 | TARGET TYPE | instance | | LOAD BALANCER ARNS | arn:aws:elasticloadbalancing:us-west-2:195750747780:loadbalancer/gwy/vpc-egress-east-west-GWLB/0b613a42d8050581 | | | | | | HEALTH CHECK PROTOCOL | HEALTH CHECK PORT | HEALTHY THRESHOLD | UNHEALTHY THRESHOLD | TIMEOUT SECONDS | INTERVAL SECONDS | | HTTPS | 6081 | 3 | 3 | 5 | 10 | | TARGETS AND TARGET HEALTH | | | | | | | TARGET ID | TARGET PORT | STATE | REASON | DESCRIPTION | | | i-0ae498b581ad025c3 | 6081 | healthy | --- | --- | | | i-0482047cec4fa3d44 | 6081 | healthy | --- | --- | | | i-0b05aa467b3b11537 | 6081 | healthy | --- | --- | | | i-00b7cba754dfc68b4 | 6081 | unhealthy | Target.Timeout | Connection to target timed out | | |

# EC2 Instances

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Region: eu-west-1 / VPC: vpc-egress-east-west-TransitVPC (3 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0a9d430a70bb92221 | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ1 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1a | PRIV IP | 10.206.0.202 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-07461bd65248866b6/VM-Series Data - AZ1 | 10.206.0.202 |  | subnet-047b36d8680df0b08(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ1) | sg-0ece74c8634d2bcbe | 0 | | eni-02cd65b1caf92ca8b/VM-Series Management - AZ1 | 10.206.0.58 |  | subnet-0efb73c4242d840c9(gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ1) | sg-009d2a9f849023fad | 1 | | eni-0f0a1393f2dad36ee/Egress - AZ1 | 10.206.0.10 | 52.208.84.158 | subnet-044b170482feebaf7(gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ1) | sg-052b322624c487107 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-09e100fc017b51e6f | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ2 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1b | PRIV IP | 10.206.0.218 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0f9fdcaaad590bed2/VM-Series Data - AZ2 | 10.206.0.218 |  | subnet-012c022e55482f0e3(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ2) | sg-0ece74c8634d2bcbe | 0 | | eni-0c82c4406ff7015f9/VM-Series Management - AZ2 | 10.206.0.74 |  | subnet-0faaa483434284bf2(gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ2) | sg-009d2a9f849023fad | 1 | | eni-0954b9bf1a0200f17/Egress - AZ2 | 10.206.0.26 | 3.248.157.14 | subnet-01172f1cc5eb6e7c8(gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ2) | sg-052b322624c487107 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0bb50fb55ec372473 | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ3 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1c | PRIV IP | 10.206.0.234 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0afeb7aad3d594177/VM-Series Data - AZ3 | 10.206.0.234 |  | subnet-08babfb693ceba8d7(gbtcloud-transit-egress-east-west-euw1-DataSubnet-AZ3) | sg-0ece74c8634d2bcbe | 0 | | eni-017d849c81e426f96/VM-Series Management - AZ3 | 10.206.0.90 |  | subnet-0929ed3d913b63e35(gbtcloud-transit-egress-east-west-euw1-MgmtSubnet-AZ3) | sg-009d2a9f849023fad | 1 | | eni-0f05872efd78df0ec/Egress - AZ3 | 10.206.0.42 | 34.253.248.85 | subnet-0e7b7fda70a4378d7(gbtcloud-transit-egress-east-west-euw1-PublicSubnet-AZ3) | sg-052b322624c487107 | 2 | |  |  |  |  |  |
| Region: eu-west-1 / VPC: vpc-ingress-TransitVPC (3 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-065a1e9a62fc6c8fb | | | | | | | NAME | vpc-ingress-VMSeries-AZ1 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1a | PRIV IP | 10.206.4.202 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-03dbb3af9a47661c0/VM-Series Data - AZ1 | 10.206.4.202 |  | subnet-0b7cc295e657bc900(gbtcloud-transit-ingress-euw1-DataSubnet-AZ1) | sg-080992c081971b7df | 0 | | eni-0f540761f25faae84/VM-Series Management - AZ1 | 10.206.4.58 |  | subnet-041a8830ec6be5eff(gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ1) | sg-0410a18e5adea3b16 | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0e2f2015210a7a043 | | | | | | | NAME | vpc-ingress-VMSeries-AZ3 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1c | PRIV IP | 10.206.4.234 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0586248ec3a22917a/VM-Series Data - AZ3 | 10.206.4.234 |  | subnet-0efe857ac9c1f277c(gbtcloud-transit-ingress-euw1-DataSubnet-AZ3) | sg-080992c081971b7df | 0 | | eni-04dfd973c9f3e0cd9/VM-Series Management - AZ3 | 10.206.4.90 |  | subnet-067c3ec94561daedc(gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ3) | sg-0410a18e5adea3b16 | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-010b766c694091022 | | | | | | | NAME | vpc-ingress-VMSeries-AZ2 | AMI | ami-03025ae850426a781 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | eu-west-1b | PRIV IP | 10.206.4.218 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-07dc6d28fa2501f75/VM-Series Data - AZ2 | 10.206.4.218 |  | subnet-04d20ca271b2037e8(gbtcloud-transit-ingress-euw1-DataSubnet-AZ2) | sg-080992c081971b7df | 0 | | eni-06cb89313d4d0a033/VM-Series Management - AZ2 | 10.206.4.74 |  | subnet-0c50807935eca55ee(gbtcloud-transit-ingress-euw1-MgmtSubnet-AZ2) | sg-0410a18e5adea3b16 | 1 | |  |  |  |  |  |
| Region: us-east-1 / VPC: vpc-ingress-TransitVPC (4 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-090c6188b0f4c8526 | | | | | | | NAME | vpc-ingress-VMSeries-AZ2 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1b | PRIV IP | 10.201.4.218 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0fb90c2501c875c58/VM-Series Data - AZ2 | 10.201.4.218 |  | subnet-09cd58c7ca6e18f78(gbtcloud-transit-ingress-use1-DataSubnet-AZ2) | sg-05771702e0bbb1754 | 0 | | eni-056d2f0243e41489d/VM-Series Management - AZ2 | 10.201.4.74 |  | subnet-0ebd346130a6a4f21(gbtcloud-transit-ingress-use1-MgmtSubnet-AZ2) | sg-01dee5b2f04991bb1 | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0319a9685c5d55130 | | | | | | | NAME | vpc-ingress-VMSeries-AZ1 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1a | PRIV IP | 10.201.4.202 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-05d867047b274d84c/VM-Series Data - AZ1 | 10.201.4.202 |  | subnet-0b43a92182056a059(gbtcloud-transit-ingress-use1-DataSubnet-AZ1) | sg-05771702e0bbb1754 | 0 | | eni-045978c57e416cbfa/VM-Series Management - AZ1 | 10.201.4.58 |  | subnet-06df68360ca86da15(gbtcloud-transit-ingress-use1-MgmtSubnet-AZ1) | sg-01dee5b2f04991bb1 | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0f0b34371a4e321c6 | | | | | | | NAME | vpc-ingress-VMSeries-AZ3 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1d | PRIV IP | 10.201.4.234 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0458bf0103980989b/VM-Series Data - AZ3 | 10.201.4.234 |  | subnet-069dca8181c1d46c7(gbtcloud-transit-ingress-use1-DataSubnet-AZ3) | sg-05771702e0bbb1754 | 0 | | eni-0882cd1849424b207/VM-Series Management - AZ3 | 10.201.4.90 |  | subnet-07126fcf9b6869e52(gbtcloud-transit-ingress-use1-MgmtSubnet-AZ3) | sg-01dee5b2f04991bb1 | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-05e2adcbe1ca07191 | | | | | | | NAME | SSH Troubleshooting Server | AMI | ami-02f3f602d23f1659d | INST TYPE / ENA SUPPORT | t3.small/YES | | AZ | us-east-1d | PRIV IP | 10.201.4.232 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | SSH Troubleshooting Server NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-07d9efbfc1438b5bc/ | 10.201.4.232 |  | subnet-069dca8181c1d46c7(gbtcloud-transit-ingress-use1-DataSubnet-AZ3) | sg-05771702e0bbb1754 sg-03d5a5b986a45a183 sg-01dee5b2f04991bb1 | 0 | |  |  |  |  |  |
| Region: us-east-1 / VPC: vpc-egress-east-west-TransitVPC (8 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-04ca9983676a3c231 | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ2 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1b | PRIV IP | 10.201.0.218 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | stopped | | vpc-egress-east-west-VMSeries-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-06ccf2462927c5122/VM-Series Data - AZ2 | 10.201.0.218 |  | subnet-06d3aae69ad09e76b(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ2) | sg-0745b4634b4d34ee9 | 0 | | eni-0ba8f3cf99894bb09/VM-Series Management - AZ2 | 10.201.0.74 |  | subnet-0896aa0ebae1ef5e4(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ2) | sg-08582a4436c53e22e | 1 | | eni-057d0079e540d047e/Egress - AZ2 | 10.201.0.26 | 54.82.127.74 | subnet-01c1e38462c29aed9(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ2) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0a650ff17d374c482 | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ1 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1a | PRIV IP | 10.201.0.202 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | stopped | | vpc-egress-east-west-VMSeries-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0adf2e6bd6fe34d92/VM-Series Data - AZ1 | 10.201.0.202 |  | subnet-08abcdb3032981389(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ1) | sg-0745b4634b4d34ee9 | 0 | | eni-037dcf5dc65fb013e/VM-Series Management - AZ1 | 10.201.0.58 |  | subnet-0206007c6c5c34387(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ1) | sg-08582a4436c53e22e | 1 | | eni-011e59c4937a8a5bc/Egress - AZ1 | 10.201.0.10 | 52.23.22.104 | subnet-06cdf28668685bb3a(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ1) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-02a604d156d4a50a3 | | | | | | | NAME | vpc-egress-east-west-VMSeries-AZ3 | AMI | ami-038af5364fe2df682 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-east-1d | PRIV IP | 10.201.0.234 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | stopped | | vpc-egress-east-west-VMSeries-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0335b147a6c8a974d/VM-Series Data - AZ3 | 10.201.0.234 |  | subnet-005c0c6cab91c08f1(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ3) | sg-0745b4634b4d34ee9 | 0 | | eni-0efee9424a2b5570a/VM-Series Management - AZ3 | 10.201.0.90 |  | subnet-027ec1fdb8d160cab(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ3) | sg-08582a4436c53e22e | 1 | | eni-062eaf327e58e6b52/Egress - AZ3 | 10.201.0.42 | 54.163.150.36 | subnet-0ac717436d1186181(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ3) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-071017ef5eeb4c869 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ3 | AMI | ami-0c607f80667dcede7 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-east-1d | PRIV IP | 10.201.0.233 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-050d3e4d65ef15231/VM-Series Data 700 - AZ3 | 10.201.0.233 |  | subnet-005c0c6cab91c08f1(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ3) | sg-0745b4634b4d34ee9 | 0 | | eni-0b7979675a39ccd82/VM-Series Management 700 - AZ3 | 10.201.0.89 |  | subnet-027ec1fdb8d160cab(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ3) | sg-08582a4436c53e22e | 1 | | eni-0cac61836ca64767c/Egress 700 - AZ3 | 10.201.0.41 | 52.55.108.76 | subnet-0ac717436d1186181(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ3) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0578d334991cdf78c | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ3-B | AMI | ami-0c607f80667dcede7 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-east-1d | PRIV IP | 10.201.0.237 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | stopped | | vpc-egress-east-west-VMSeries700-AZ3-B NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0792a269aecf42244/VM-Series Data 700 - AZ3 - B - [ 2nd Node ] | 10.201.0.237 |  | subnet-005c0c6cab91c08f1(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ3) | sg-0745b4634b4d34ee9 | 0 | | eni-0f392c59d3154fc1f/VM-Series Management 700 - AZ3 - B - [ 2nd Node ] | 10.201.0.93 |  | subnet-027ec1fdb8d160cab(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ3) | sg-08582a4436c53e22e | 1 | | eni-0ecd1ad9c018bb7fa/Egress 700 - AZ3 - B - [ 2nd Node ] | 10.201.0.45 | 44.194.89.232 | subnet-0ac717436d1186181(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ3) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-04df721cb262df221 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ1 | AMI | ami-0c607f80667dcede7 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-east-1a | PRIV IP | 10.201.0.201 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-04443b6b4f4fe9b4a/VM-Series Data 700 - AZ1 | 10.201.0.201 |  | subnet-08abcdb3032981389(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ1) | sg-0745b4634b4d34ee9 | 0 | | eni-0ff97f439b5fac326/VM-Series Management 700 - AZ1 | 10.201.0.57 |  | subnet-0206007c6c5c34387(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ1) | sg-08582a4436c53e22e | 1 | | eni-010db0c0a65ec2a09/Egress 700 - AZ1 | 10.201.0.9 | 18.211.34.250 | subnet-06cdf28668685bb3a(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ1) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-08db73a64101064d9 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ2 | AMI | ami-0c607f80667dcede7 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-east-1b | PRIV IP | 10.201.0.217 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-07f545e2d9f1c38a5/VM-Series Data 700 - AZ2 | 10.201.0.217 |  | subnet-06d3aae69ad09e76b(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ2) | sg-0745b4634b4d34ee9 | 0 | | eni-081d16523205e8ebd/VM-Series Management 700 - AZ2 | 10.201.0.73 |  | subnet-0896aa0ebae1ef5e4(gbtcloud-transit-egress-east-west-use1-MgmtSubnet-AZ2) | sg-08582a4436c53e22e | 1 | | eni-0ad3b5709864559b5/Egress 700 - AZ2 | 10.201.0.25 | 54.156.81.227 | subnet-01c1e38462c29aed9(gbtcloud-transit-egress-east-west-use1-PublicSubnet-AZ2) | sg-0553ef4f38bf13091 | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0af810c57bc508c6f | | | | | | | NAME | USE1NPLAPLVAA01 | AMI | ami-04896e33c24f8ec34 | INST TYPE / ENA SUPPORT | m5.4xlarge/YES | | AZ | us-east-1a | PRIV IP | 10.201.0.200 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | stopped | | USE1NPLAPLVAA01 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0faabd5fb05808604/Primary network interface | 10.201.0.200 |  | subnet-08abcdb3032981389(gbtcloud-transit-egress-east-west-use1-DataSubnet-AZ1) | sg-0316292a888ef84bf sg-0dbd0cb854378bdc6 | 0 | |  |  |  |  |  |
| Region: us-west-2 / VPC: vpc-ingress-TransitVPC (3 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-04dd921823ef6b565 | | | | | | | NAME | vpc-ingress-VMSeries-AZ3 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-west-2c | PRIV IP | 10.228.4.234 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-02a778b3809cdbeea/VM-Series Data - AZ3 | 10.228.4.234 |  | subnet-0cda254219dfbdc12(gbtcloud-transit-ingress-usw2-DataSubnet-AZ3) | sg-08801f2668550b9a6 | 0 | | eni-06c1b70aecc2a81e5/VM-Series Management - AZ3 | 10.228.4.90 |  | subnet-0fa7f4bef4db50282(gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ3) | sg-083652d7e289a206a | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-020d853d4a8d15f9e | | | | | | | NAME | vpc-ingress-VMSeries-AZ1 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-west-2a | PRIV IP | 10.228.4.202 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-045f8f1613a678206/VM-Series Data - AZ1 | 10.228.4.202 |  | subnet-0cc312e8737099d62(gbtcloud-transit-ingress-usw2-DataSubnet-AZ1) | sg-08801f2668550b9a6 | 0 | | eni-01a7aa607e8a90356/VM-Series Management - AZ1 | 10.228.4.58 |  | subnet-09bcaa5b1386feb2e(gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ1) | sg-083652d7e289a206a | 1 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-056c44368214abe8f | | | | | | | NAME | vpc-ingress-VMSeries-AZ2 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5.xlarge/YES | | AZ | us-west-2b | PRIV IP | 10.228.4.218 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-ingress-VMSeries-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0b21bb321741f82ad/VM-Series Data - AZ2 | 10.228.4.218 |  | subnet-00caacfc0213289c6(gbtcloud-transit-ingress-usw2-DataSubnet-AZ2) | sg-08801f2668550b9a6 | 0 | | eni-0ac8bd385f2ddee5f/VM-Series Management - AZ2 | 10.228.4.74 |  | subnet-0ec8a9d381c3104a8(gbtcloud-transit-ingress-usw2-MgmtSubnet-AZ2) | sg-083652d7e289a206a | 1 | |  |  |  |  |  |
| Region: us-west-2 / VPC: vpc-egress-east-west-TransitVPC (3 Instances) |  |  |  |  |  |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0b05aa467b3b11537 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ3 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-west-2c | PRIV IP | 10.228.0.233 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ3 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-07c778d5907f5daae/VM-Series Data 700 - AZ3 | 10.228.0.233 |  | subnet-0038de275ab5144d8(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ3) | sg-0526cb6fbaec4c1b0 | 0 | | eni-0b467793ce01f6aba/VM-Series Management 700 - AZ3 | 10.228.0.89 |  | subnet-0d7a07d117c0d5af6(gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ3) | sg-02cede6aee227f247 | 1 | | eni-0d6251aad8acaa51b/Egress 700 - AZ3 | 10.228.0.41 | 54.69.178.32 | subnet-0b1b9f9bc74795934(gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ3) | sg-0e8c49685c1dca9bc | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0482047cec4fa3d44 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ1 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-west-2a | PRIV IP | 10.228.0.201 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ1 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0425178c1c68bdee7/VM-Series Data 700 - AZ1 | 10.228.0.201 |  | subnet-0d73be1ad800b7008(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ1) | sg-0526cb6fbaec4c1b0 | 0 | | eni-00c1f8a730fbbe154/VM-Series Management 700 - AZ1 | 10.228.0.57 |  | subnet-00a22a642d83879be(gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ1) | sg-02cede6aee227f247 | 1 | | eni-04a8cb4cb379fbc6c/Egress 700 - AZ1 | 10.228.0.9 | 44.232.172.52 | subnet-08cbba5a6f687cc44(gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ1) | sg-0e8c49685c1dca9bc | 2 | |  |  |  |  |  |
|  | | | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | INSTANCE ID: i-0ae498b581ad025c3 | | | | | | | NAME | vpc-egress-east-west-VMSeries700-AZ2 | AMI | ami-053115e5dc458e709 | INST TYPE / ENA SUPPORT | m5n.4xlarge/YES | | AZ | us-west-2b | PRIV IP | 10.228.0.217 | PUB IP |  | | PLATFORM | Linux/UNIX | ARCHITECTURE | x86\_64 | STATE | running | | vpc-egress-east-west-VMSeries700-AZ2 NETWORK INTERFACES | | | | | | | INT ID/DESCRIPTION | PRIV IPS | PUB IP | SUBNET | SG IDS | DEV INDEX | | eni-0d0d95d0adaf8d4e3/VM-Series Data 700 - AZ2 | 10.228.0.217 |  | subnet-0334b4095a7630a4f(gbtcloud-transit-egress-east-west-usw2-DataSubnet-AZ2) | sg-0526cb6fbaec4c1b0 | 0 | | eni-067d1b6f83012ddce/VM-Series Management 700 - AZ2 | 10.228.0.73 |  | subnet-001e537abca8620c8(gbtcloud-transit-egress-east-west-usw2-MgmtSubnet-AZ2) | sg-02cede6aee227f247 | 1 | | eni-094929c0074c7e047/Egress 700 - AZ2 | 10.228.0.25 | 34.209.159.206 | subnet-06ff9bd4330a6e906(gbtcloud-transit-egress-east-west-usw2-PublicSubnet-AZ2) | sg-0e8c49685c1dca9bc | 2 | |  |  |  |  |  |